***Welding Health and Safety Procedures***

**Info**

***Protective mats***

*Welding is a term used for joining metal to metal this can consist of multiple processes but not limited to (GMAW, MMAW, GTAW). But not limited to.*

*Welding is a extremely dangerous procedure there is a huge risk of fires.*

*What we do to combat Fire Risks.*

*Examples (not Limited to)*

* *1x L fire extinguisher*
* *1x L Fire extinguisher*
* *Site assessment*
* *Risk Assessment*
* *Hose ready (Where available)*
* *Protective coverings( Boards, drop sheets)*

*Practical steps Takin*

*Sparks/Fires*

***Protective mats placed in ensure gorund is not dmaged from grinding sparks or welding.***

***Windows all attempts are made to ensure that no grinding sparks reach windows***